Neck angle pipeline

* Load vtu files from the last cycle
* Slice from the top to bottom. Crucial that Slice1 is top etc.

Macro:

Applies integratevariables to each slice. Reads the intvar point which is the centroid. Computes artificial lines, which the angle is then calculated. Line12 and line23 have the angle alpha, while line23 and line34 have the angle beta.